{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","Sheet3"],"not_rendered":{"images":5},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":8,"rows_kept":7,"merged":[[0,0,0,7],[1,0,1,7],[3,1,5,1],[6,0,6,6]]}
["市场询价情况表"]
["木栈道改造"]
["序号","询价单位","品牌、型号及参数","图例","单位","数量","单价/元","金额/元"]
[1,null,"重竹木地板规格：L*137*18厚户外高耐竹地板留缝5厘专用金属扣件固定。铺设整齐牢固。            框架龙骨铺设：L*50*50*5厚热镀锌方钢管龙骨，间距375mm，50*50*3厚热镀锌角钢固定(含旧栈道拆除及垃圾清运）",null,"平方米",1850]
[2,null,"长条椅规格：2.0厚304不锈钢架构+3.2CM*5.5CM的防腐防火防腐木板椅面，每条长2M*宽0.4M*高0.45M。根据现场实际情况安装（约260条）。",null,"米",510]
[3,null,"栏杆规格、形状：详见附件",null,"米",380]
["合计",{"$nulls":6},{"$f":"SUM(H4:H6)","v":0}]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}