{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":3,"rows_kept":3,"flags":["formulas_cached_only"]}
["名称","规格参数","产品样式"]
["白胡桃纹760矮柜对开门","尺寸：长900MM*宽400MM*高760MM                   材质要求：厚度1.2MM SPCC冷轧钢板                           喷涂工艺：采用静电喷粉保证环保无味             需配备1个锁2把备用钥匙"]
["白胡桃纹1090矮柜对开门","尺寸：长900MM*宽400MM*高1090MM                 材质要求：厚度1.2MM SPCC冷轧钢板                           喷涂工艺：采用静电喷粉保证环保无味                需配备1个锁2把备用钥匙"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}