{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":2,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":4,"n_cols":7,"rows_kept":4,"flags":["formulas_cached_only"]}
["名称","规格参数","安装场地","单价（元）","单位","数量"]
["人脸识别感应玻璃门","品牌自动感应人脸识别门禁系统一体机，玻璃门尺寸约2.2米*2.55米，含10厘钢化玻璃、加厚铝通方管、全包边等一切安装所需辅材，包安装，质保2年，按实结算",null,8000,"个",1]
["人脸识别感应玻璃门","品牌自动感应人脸识别门禁系统一体机，玻璃门尺寸约2.45米*2.5米，含10厘钢化玻璃、加厚铝通方管、全包边等一切安装所需辅材，包安装，质保2年，按实结算",null,8000,"个",1]
[{"$nulls":6},16000]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}